Packet Tracer - Use Ping and Traceroute to Test Network Connectivity

# Addressing Table

| **Device** | **Interface** | **IP Address / Prefix** | | **Default Gateway** |
| --- | --- | --- | --- | --- |
| R1 | G0/0 | 2001:db8:1:1::1/64 | | N/A |
| *R1* | G0/1 | 10.10.1.97 | 255.255.255.224 | N/A |
| *R1* | S0/0/1 | 10.10.1.6 | 255.255.255.252 | N/A |
| *R1* | *S0/0/1* | 2001:db8:1:2::2/64 | | *N/A* |
| *R1* | *S0/0/1* | fe80::1 | | *N/A* |
| R2 | S0/0/0 | 10.10.1.5 | 255.255.255.252 | N/A |
| *R2* | *S0/0/0* | 2001:db8:1:2::1/64 | | *N/A* |
| *R2* | S0/0/1 | 10.10.1.9 | 255.255.255.252 | N/A |
| *R2* | *S0/0/1* | 2001:db8:1:3::1/64 | | *N/A* |
| *R2* | *S0/0/1* | fe80::2 | | *N/A* |
| R3 | G0/0 | 2001:db8:1:4::1/64 | | N/A |
| *R3* | G0/1 | 10.10.1.17 | 255.255.255.240 | N/A |
| *R3* | S0/0/1 | 10.10.1.10 | 255.255.255.252 | N/A |
| *R3* | *S0/0/1* | 2001:db8:1:3::2/64 | | *N/A* |
| *R3* | *S0/0/1* | fe80::3 | | *N/A* |
| PC1 | NIC | 10.10.1.98 | 255.255.255.224 | 10.10.1.97 |
| PC2 | NIC | 2001:DB8:1:1::2 | | FE80::1 |
| PC3 | NIC | 10.10.1.18 | 255.255.255.240 | 10.10.1.17 |
| PC4 | NIC | 2001:DB8:1:4::2 | | FE80::2 |

# Objectives

**Part 1: Test and Restore IPv4 Connectivity**

**Part 2: Test and Restore IPv6 Connectivity**

# Scenario

There are connectivity issues in this activity. In addition to gathering and documenting information about the network, you will locate the problems and implement acceptable solutions to restore connectivity.

**Note:** The user EXEC password is **cisco**. The privileged EXEC password is **class**.

# Instructions

## Test and Restore IPv4 Connectivity

### Use ipconfig and ping to verify connectivity.

* + - 1. Click **PC1** and open the **Command Prompt**.
      2. Enter the **ipconfig /all** command to collect the IPv4 information. Complete the **Addressing Table** with the IPv4 address, subnet mask, and default gateway.
      3. Click **PC3** and open the **Command Prompt**.
      4. Enter the **ipconfig /all** command to collect the IPv4 information. Complete the **Addressing Table** with the IPv4 address, subnet mask, and default gateway.
      5. Use the **ping** command to test connectivity between **PC1** and **PC3**. The ping should fail.

### Locate the source of connectivity failure.

* + - 1. From **PC1**, enter the necessary command to trace the route to **PC3**.

#### Question:

What is the last successful IPv4 address that was reached?

10.10.1.97

* + - 1. The trace will eventually end after 30 attempts. Enter **Ctrl**+**C** to stop the trace before 30 attempts.
      2. From **PC3**, enter the necessary command to trace the route to **PC1**.

#### Question:

What is the last successful IPv4 address that was reached?

10.10.1.17

* + - 1. Enter **Ctrl**+**C** to stop the trace.

*Open configuration window*

* + - 1. Click **R1**. Press **ENTER** and log in to the router.
      2. Enter the **show ip interface brief** command to list the interfaces and their status. There are two IPv4 addresses on the router. One should have been recorded in Step 2a.

#### Question:

What is the other?

10.10.1.6

* + - 1. Enter the **show ip route** command to list the networks to which the router is connected. Note that there are two networks connected to the **Serial0/0/1** interface.

#### Question:

What are they?

10.10.1.4/30 and 10.10.1.6/32

* + - 1. Repeat steps 2e through 2g with **R3** and record your answers.

10.10.1.17, 10.10.1.8/30 and 10.10.1.10/32

* + - 1. Click **R2**. Press **ENTER** and log into the router.
      2. Enter the **show ip interface brief** command and record your addresses. 10.10.1.2, 10.10.1.9

***Type your addresses here.***

* + - 1. Run more tests if it helps visualize the problem. Simulation mode is available.

*Close configuration window*

### Propose a solution to solve the problem.

Compare your answers in Step 2 to the documentation you have available for the network.

#### Question:

What is the error?

The IP address of S/0/0/0 in the table is 10.10.1.5 but the IP of port S/0/0/0 in the R2 router is 10.10.1.9.

What solution would you propose to correct the problem?

Configure the R2 router’s S0/0/0 port and change its IP from 10.10.1.9 to 10.10.15 .

### Implement the plan.

Implement the solution you proposed in Step 3b.

### Verify that connectivity is restored.

* + - 1. From **PC1** test connectivity to **PC3**.
      2. From **PC3** test connectivity to **PC1**.

#### Question:

Is the problem resolved?

Problem is solved

### Document the solution.

## Test and Restore IPv6 Connectivity

### Use ipv6config and ping to verify connectivity.

* + - 1. Click **PC2** and open the **Command Prompt**.
      2. Enter the **ipv6config /all** command to collect the IPv6 information. Complete the **Addressing Table** with the IPv6 address, subnet prefix, and default gateway.
      3. Click **PC4** and open the **Command Prompt**.
      4. Enter the **ipv6config /all** command to collect the IPv6 information. Complete the **Addressing Table** with the IPv6 address, subnet prefix, and default gateway.
      5. Test connectivity between **PC2** and **PC4**. The ping should fail.

### Locate the source of connectivity failure.

* + - 1. From **PC2**, enter the necessary command to trace the route to **PC4**.

#### Question:

What is the last successful IPv6 address that was reached?

2001:DB8:1:3::2

* + - 1. The trace will eventually end after 30 attempts. Enter **Ctrl**+**C** to stop the trace before 30 attempts.
      2. From **PC4**, enter the necessary command to trace the route to **PC2**.

#### Question:

What is the last successful IPv6 address that was reached?

No IPv6 address was reached.

* + - 1. Enter **Ctrl**+**C** to stop the trace.
      2. Click **R3**. Press **ENTER** and log in to the router.
      3. Enter the **show ipv6 interface brief** command to list the interfaces and their status. There are two IPv6 addresses on the router. One should match the gateway address recorded in Step 1d.

#### Question:

Is there a discrepancy?

No discrepancy

* + - 1. Run more tests if it helps visualize the problem. Simulation mode is available.

### Propose a solution to solve the problem.

Compare your answers in Step 2 to the documentation you have available for the network.

#### Question:

What is the error?

The default gateway of PC4 and IP address of R3 were not the same. ***asd***

What solution would you propose to correct the problem?

Change IPv6 gateway address of PC4 from its IP configuration.

### Implement the plan.

Implement the solution you proposed in Step 3b.

### Verify that connectivity is restored.

* + - 1. From **PC2** test connectivity to **PC4**.
      2. From **PC4** test connectivity to **PC2**.

#### Question:

Is the problem resolved?

The problem has been solved

### Document the solution.

Changing the Default gateway from FE80::2 to FE80::3 solved the problem of PC4.